/1

/100 s

/101 s

/100 c

/101 s

/102 s

/101 c

/1

/100 s

Emitter

Collector

Host

Sprocess

Wprocess

Wprocess

Mprocess

/100 s

/1

/1

/1

Channels used to initiate each worker node; use channel number 1

Bi-drectional channels with input ends identified

Uni-drectional channels with input ends identified